{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["项目报价"],"not_rendered":{"images":13},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"项目报价","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"merged":[[0,0,0,8],[2,0,2,8],[22,0,22,8],[26,0,27,0],[37,0,37,8],[41,0,42,0],[52,0,52,8],[53,1,53,8]],"flags":["formulas_cached_only"]}
["泰州体育公园比赛照明投标清单"]
["序号","产品名称","品牌","品牌及型号","图例","数量","单位","单价","合计"]
["体育场照明灯具清单"]
[1,"场地投光灯（金卤灯）","飞利浦","mvf403 CZ 2000W ",null,256,"套"]
[2,"LED观众席投光灯","飞利浦","BVP432 LED272CW 200W SMB",null,136,"套"]
[3,"LED应急照明投光灯","飞利浦","BVP433 LED413/CW  305W SMB   ",null,50,"套"]
[4,"12路开关模块","飞利浦","DDRC1220FR-GL",null,32,"套"]
[5,"4路开关模块","飞利浦","DDRC420",null,2,"套"]
[6,"以太网关","飞利浦","PDEB",null,2,"套"]
[7,"直流电源","明纬","HDR-100-24",null,6,"套"]
[8,"电源冗余模块","明纬","DRDN20-24",null,3,"套"]
[9,"以太网交换机",null,"24口、24千兆电口+4万兆光口WEB网管交换机",null,3,"套"]
[10,"光缆熔接盒",null,"四口",null,2,"套"]
[11,"光缆熔接盒",null,"八口",null,1,"套"]
[12,"触摸屏面板及模块控制","飞利浦","PDTS",null,1,"套"]
[13,"以太网关","飞利浦","PDEG",null,1,"套"]
[14,"控制箱开关",null,"紧急启动（安装于配电箱表面）",null,5,"套"]
[15,"总控软件","飞利浦","EnvisionManager software",null,1,"套"]
[16,"主控电脑（含桌椅）","DELL","CPU i710700,硬盘容量256G,内存16G，win10操作系统",null,1,"套"]
[17,"网络机柜","600*800*2000mm，优质冷轧钢板、经过脱脂、酸洗、磷化、静电喷塑工艺价格、加大热排量、前后门采用六角式蜂窝是网孔、覆铝锌立柱，坚固耐用","W600mm x D800mm x H2000mm，带PDU及风冷机组",null,3,"套"]
[18,"第三方检测费",null,"暂定按实际开票金额结算",null,1,"次"]
[null,"小计",{"$nulls":6},0]
["体育馆照明灯具清单"]
[1,"体育馆投光灯（金卤灯）","飞利浦 ","mvf403 CZ 1000W",null,248,"套"]
[2,"LED观众席投光灯 ","飞利浦","BVP432 LED272CW 200W SMB",null,60,"套"]
[3,"LED应急投光灯","飞利浦","BVP431  LED92/CW  70W SMB ",null,44,"套"]
[4,"LED训练场投光灯","飞利浦","BVP433 LED517/CW 380W",null,20,"套"]
[null,"LED训练场投光灯","飞利浦","BVP432 LED161/CW  120W SMB ",null,6,"套"]
[5,"带屏显控制面板","飞利浦"," 十键面板",null,2,"套"]
[6,"12路开关模块","飞利浦","DDRC1220FR-GL",null,15,"套"]
[7,"4路开关模块","飞利浦","DDRC420",null,2,"套"]
[8,"转换器","飞利浦","DTK622",null,1,"套"]
[9,"主控电脑（含桌椅）","DELL","CPU i710700,硬盘容量256G,内存16G，win10操作系统",null,1,"套"]
[10,"网络机柜","600*800*2000mm，优质冷轧钢板、经过脱脂、酸洗、磷化、静电喷塑工艺价格、加大热排量、前后门采用六角式蜂窝是网孔、覆铝锌立柱，坚固耐用","W600mm x D600mm x H2000mm，带PDU及风冷机组",null,1,"套"]
[11,"总控软件","飞利浦","EnvisionManager software",null,1,"套"]
[12,"第三方检测费",null,"暂定按实际开票金额结算",null,1,"次"]
[null,"小计"]
["游泳馆照明灯具清单"]
[1,"游泳馆投光灯(金卤灯) ","飞利浦","mvf403 CZ 1000W ",null,112,"套"]
[2,"LED观众席投光灯 ","飞利浦","BVP432 LED272CW 200W SMB",null,20,"套"]
[3,"LED应急投光灯","飞利浦","BVP431  LED92/CW  70W SMB ",null,16,"套"]
[4,"LED训练场地投光灯","飞利浦","BVP433 LED517/CW 380W",null,14,"套"]
[null,"LED训练场地投光灯","飞利浦","BVP431  LED92/CW  70W SMB ",null,4,"套"]
[5,"带屏显控制面板","飞利浦"," 十键面板",null,2,"套"]
[6,"12路开关模块","飞利浦","DDRC1220FR-GL",null,8,"套"]
[7,"主控电脑（含桌椅）","DELL","CPU i710700,硬盘容量256G,内存16G，win10操作系统",null,1,"套"]
[8,"网络机柜","600*800*2000mm，优质冷轧钢板、经过脱脂、酸洗、磷化、静电喷塑工艺价格、加大热排量、前后门采用六角式蜂窝是网孔、覆铝锌立柱，坚固耐用","W600mm x D600mm x H2000mm，带PDU及风冷机组",null,1,"套"]
[9,"总控软件","飞利浦","EnvisionManager software",null,1,"套"]
[10,"转换器","飞利浦","DTK622",null,1,"套"]
[11,"第三方检测费",null,"暂定按实际开票金额结算",null,1,"次"]
[null,"小计"]
[null,"总价"]
[]
["备注","1、本报价含增值税发票，含运费。"]